> Marker Menu
> Key Sequence: Marker

> Marker Menu (1 of 2)

> Marker Setup
> Select (1-8) M#
> Edit
> Type
> M# (On Off)
> Display (Mkr + Table, Mkr Only, Off)
> Press to open display options.
> Mkr+Table: Displays both the markers that are on and marker table.
> Mkr Only: Displays markers that are on, hides the marker table.
> Off: Hides all markers and the marker table.
> Marker Preset
> Turns off all markers except for Marker 1. Sets Marker 1 location to the middle of the sweep.

> Marker Menu (Continued)
> Key Sequence: Marker

> Marker Menu (2 of 2)

> Marker Search:
> Tracking (On Off)
> When turned On, the active marker becomes a tracking marker and defaults to tracking the peak. To track Valleys, press the Marker to Valley button after turning on Tracking. The Search settings can all be applied to a Marker with Tracking either On or Off.
> Marker to Peak
> Marker to Valley
> Markers 5, 6, 7, and 8 can perform a special Marker search to find the Peak or Valley between two other markers.
> When Marker 5 or Marker 7 is Active:
> Valley Between M1 & M2: Places Marker 5 or 7 on the lowest signal amplitude between Marker 1 and Marker 2.
> When Marker 6 or Marker 8 is Active:
> Peak Between M3 & M4: Places Marker 6 or 8 on the highest signal amplitude between Marker 3 and Marker 4.
> Valley Between M3 & M4: Places Marker 6 or 8 on the lowest signal amplitude between Marker 3 and Marker 4.