> Calibration Procedure

> 1. | Press the Freq/Dist main menu key and enter the appropriate frequency range.

> 2. | Press the Calibration main menu key, then press Start Calibration.

> 3. | Select either Standard or Flex.

> 4. | Select the Cal Method to be OSL, InstaCal, Transmission (Ext. Sensor), or OSL + Transmission (Ext. Sensor).

> 5. | Press Measure and follow the on-screen instructions (Figure: Calibration Setup OSL Cal).

> 6. | Verify that the calibration has been completed by confirming that the Cal Status message is now displaying the following:

> • | Cal Status OK (RFP1) or iCal Status OK (RFP1) for 1-port standard or flex reflection calibrations using either OSL or InstaCal.

> • | Cal Status OK (TRES) or iCal Status OK (TRES) for Transmission standard or flex calibrations

> • | Cal Status OK (2PES) or iCal Status OK (2PES) for combined OSL + Transmission standard or flex calibrations

> 7. | The calibration correction factor will now be applied to the measurements.

> Calibration Setup OSL Cal