> Internal Power Meter
> Overview
> Introduction
> General Measurement Setup
> Connection and Offset
> Set the Measurement Frequency
> Setting the Amplitude
> Changing the Display Units
> Displaying Relative Power
> Setting Upper and Lower Limits
> Average Menu Options
> Calibration
> Power Meter Menus
> Frequency Menu
> Amplitude Menu
> Calibration Menu
> Average Menu
> Limit Menu
> Sweep Menu
> Trace Menu
> Other Menus Keys
> Overview
> This chapter provides an overview of power meter measurements and how to set up the instrument to use the power meter. The power meter displays measured input power at the power meter connector in dBm and Watts or relative power in dB and percentage. No external sensor is required or used. The Power Meter frequency span is fixed to receive RF frequencies from 50 MHz to 4 GHz.

> Note | Check the graph title in the top right of the display to confirm that the instrument is in Power Meter mode. If necessary, press the Menu key to change modes.