> Calibrate Menu
> Key Sequence: Calibration

> Calibration Menu

> Start Calibration
> Press this submenu key and follow the instruction on screen.
> Measure: Starts the calibration process.
> Cal Method: Select one of the choices presented – OSL, InstaCal, Transmission (Ext. Sensor), or OSL + Transmission (Ext. Sensor). Refer to Calibration Methods.
> Cal Type: Toggles between Standard Cal and Flex Cal. See Table: Summary of Calibration Methods and Tools for details.
> Cal Info
> Displays information about the current settings and active cal settings. Refer to Figure: Calibration Information.
> Cal Correction On Off: Determines whether the active cal is applied to the current measurement.