> Average Menu
> Key Sequence: Average

> High Accuracy Power Meter Average Menu

> Running Average
> Sets the number of measurements used in calculating the average. Also sets the number of measurements made when Average Mode if set to Single and Run/Hold is toggled from Hold to Run. Enter the desired number by using the keypad, the rotary knob, or the Up/Down arrow keys. Press Enter to set, or press Esc to restore the previous setting.
> Max Hold
> Setting Max Hold to On will only display the maximum power level. Turning Max Hold Off will display the current power level.
> Run/Hold
> Toggles between Run and Hold. When in Hold mode, pressing this key starts the measurements and provides a trigger. When in the Run mode, pressing this key pauses the sweep.
> Average Mode
> Toggles between single measurement and continuous measurements. In Single, each measurement (or series of measurements if Running Average is greater than 1) must be activated by the Run/Hold key.