> Setting Upper and Lower Limits
> Maximum and minimum limits can be set as follows:

> 1. | Press the Limit main menu key and set Limit to On.

> 2. | Press the Upper Value submenu key and use the keypad, Up/Down arrow keys, or the rotary knob to set the desired upper limit. Then press Enter.

> 3. | Press the Lower Value submenu key and use the keypad, Up/Down arrow keys, or the rotary knob to set the desired upper limit. Then press Enter.

> The needle color and color of the numeric power level displayed below the graph change based on the current limit settings:

> • | Yellow needle, White text: Limits are turned off.

> • | Green need and text: Limits are on and the current power level value is within limits.

> • | Red needle and text: Limits are on and the current power level is not within limits.

> Refer to Figure: Limit Setting Display Changes for examples of each condition.

> Limit Setting Display Changes