> Soft Carrying Case
> The soft carrying case ( Figure: Site Master in the Soft Carrying Case) includes a detachable and adjustable carrying shoulder strap, which is connected to the D-rings of the case. For convenient use, connect the shoulder strap to opposite corners of the case and wear the strap around the neck with the unit hanging at waist height (Figure: Shoulder Strap).

> Site Master in the Soft Carrying Case

> Shoulder Strap

> To install the Site Master into the soft carrying case:

> 1. | Fully close the front panel of the soft carrying case and place the case face down on a stable surface.

> 2. | Open the zipper closest to the D-rings on the sides and bottom of the soft case to install Site Master.

> 3. | Insert the instrument face down into the case.

> 4. | Close the zipper to secure the Site Master.

> 5. | Turn the soft case over and open the front panel of the case to use the Site Master.

> 6. | A tethered stylus pen to use with the touchscreen is stored inside the soft case on the top panel, near the RF ports. Store the stylus pen in the sleeve when not in use. Replacement stylus pens with the coiled tether cord are available from Anritsu. Refer to the Site Master data sheet (11410-00616).

> Note | The grey nylon pull tab at the rear bottom of the case opens the tilt bail support panel. Adjust the open tilt angle with the hook-and-loop fastener strap. This support panel also contains two storage pockets that provide convenient and secure storage for calibration components and adapters.