> Limit Menu
> Key Sequence: Limit or Limit (6)

> High Accuracy PM (MA24105A) Limit Menu

> Limit
> Turns the limits On or Off.
> Fwd Upper Value
> Sets the forward measurement upper limit (displayed as red hash marks). Enter the desired number by using the keypad, the rotary knob, or the Up/Down arrow keys. If the keypad was used to enter new values, press Enter to set the new setting or press the Esc button to restore the previous setting.
> Fwd Lower Value
> Sets the forward measurement lower limit (displayed as red hash marks). Enter the desired number by using the keypad, the rotary knob, or the Up/Down arrow keys. If the keypad was used to enter new values, press Enter to set the new setting or press the Esc button to restore the previous setting.
> Rev Upper Value
> Sets the reverse measurement upper limit. Enter the desired number by using the keypad, the rotary knob, or the Up/Down arrow keys. If the keypad was used to enter new values, press Enter to set the new setting or press the Esc button to restore the previous setting.
> Rev Lower Value
> Sets the reverse measurement lower limit. Enter the desired number by using the keypad, the rotary knob, or the Up/Down arrow keys. If the keypad was used to enter new values, press Enter to set the new setting or press the Esc button to restore the previous setting.

> Sweep Menu
> This menu is not available in High Accuracy Power Meter measurement mode.
> Trace Menu
> This menu is not available in High Accuracy Power Meter measurement mode.