> Measurement Setup
> This section describes how to set up the Cable and Antenna parameters, markers, and limit lines.
> Frequency
> Setting up the Measurement Frequency using Start and Stop Frequencies

> 1. | Press the Freq/Dist main menu key then Frequency if the menu is collapsed.

> 2. | Press the Start Freq submenu key and enter the start frequency using the Up/Down arrow keys, rotary knob or keypad. When using the keypad, the button labels change to GHz, MHz, kHz, and Hz. Press the appropriate unit key to complete the entry.

> 3. | Press Stop Freq and enter the stop frequency.

> Distance

> 1. | Press the Freq/Dist main menu key and then Distance if the menu is collapsed.

> 2. | Press the Start Distance submenu key and enter the start distance using the Up/Down arrow keys, rotary knob or keypad. When entering a distance using the keypad, press the unit key to complete the entry.

> 3. | Press Stop Dist and enter the stop distance.