> Video Inspection Probe (VIP)
> Introduction
> Setup and Operation Summary
> VIP Setup
> Connect the VIP
> Launch the VIP Application
> VIP Test Settings
> Operation
> VIP Image Analysis
> VIP Reporting
> VIP Menus
> Setup Menu
> Measurement Menu
> File Menu
> Report Menu
> Introduction
> Signal degradation may occur as a result of a dirty or damaged optic fiber ferrule endface. The Site Master S331L supports an application that lets you inspect fiber optic terminations, using a Video Inspection Probe (VIP) such as Anritsu Model G0306A. See Figure: Anritsu G0306A Video Inspection Probe. The captured image and analysis results help determine if a connector should be cleaned or replaced. Pass/Fail evaluations are made in accordance with the IEC61300-3-35 standard. You can also save the data to file and generate test reports.

> Anritsu G0306A Video Inspection Probe