> Cable & Antenna Analyzer Mode Commands
> :CALCulate#:LIMit:LOWer:SEGMent:ADD <StartX><StopX><StartY><StopY>
> :CALCulate#:LIMit:LOWer:SEGMent:DELete
> :CALCulate#:LIMit:LOWer:SEGMent:EDIT <StartX><StopX><StartY><StopY>
> :CALCulate#:LIMit:LOWer:SEGMent:STARt:X <value>
> :CALCulate#:LIMit:LOWer:SEGMent:STARt:Y <amplitude>
> :CALCulate#:LIMit:LOWer:SEGMent:STOP:X <value>
> :CALCulate#:LIMit:LOWer:SEGMent:STOP:Y <amplitude>
> :CALCulate#:LIMit:LOWer:Y <amplitude>{dB,s|ms|ns|ps}
> :CALCulate#:LIMit:LOWer[:STATe] OFF|ON|0|1
> :CALCulate#:LIMit:UPPer:SEGMent:ADD <StartX><StopX><StartY><StopY>
> :CALCulate#:LIMit:UPPer:SEGMent:DELete
> :CALCulate#:LIMit:UPPer:SEGMent:EDIT <StartX><StopX><StartY><StopY>
> :CALCulate#:LIMit:UPPer:SEGMent:STARt:X <value>
> :CALCulate#:LIMit:UPPer:SEGMent:STARt:Y <amplitude>
> :CALCulate#:LIMit:UPPer:SEGMent:STOP:X <value>
> :CALCulate#:LIMit:UPPer:SEGMent:STOP:Y <amplitude>
> :CALCulate#:LIMit:UPPer:Y <amplitude>{dB,s|ms|ns|ps}
> :CALCulate#:LIMit:UPPer[:STATe] OFF|ON|0|1
> :CALCulate:LIMit:ALARm OFF|ON|0|1
> :CALCulate:LIMit:LOWer:SEGMent:ACTive <Index>
> :CALCulate:LIMit:MESSage OFF|ON|0|1
> :CALCulate:LIMit:MODe
> :CALCulate:LIMit:PRESet
> :CALCulate:LIMit:TYPE 0|1
> :CALCulate:LIMit:UPPer:SEGMent:ACTive <Index>
> :CALCulate:LIMit:VALue <amplitude>{dB}
> :CALCulate:LIMit[:STATe] OFF|ON|0|1
> :CALCulate:MARKer#:PEAK
> :CALCulate:MARKer#:PEAK:BOUNded
> :CALCulate:MARKer#:TRACking PEAK|VALLey|BNDPeak|BNDValley|OFF
> :CALCulate:MARKer#:TYPE REFerence|DELTa
> :CALCulate:MARKer#:VALLey
> :CALCulate:MARKer#:VALLey:BOUNded
> :CALCulate:MARKer#:X <value>{Hz|kHz|MHz|GHz,m|cm|mm,ft}
> :CALCulate:MARKer#[:STATe] OFF|ON|0|1
> :CALCulate:MARKer:DISPlay MKRTable|MKRonly|AOFF
> :CALCulate:MARKer:PRESet
> :CALCulate:MATH:FUNCtion NONE|SUBTraction|ADDition|AVERage
> :CALCulate:MATH:MEMorize
> :CALCulate:TRANsform:DISTance:CABLoss <cable-loss>{ dB/m,dB/ft}
> :CALCulate:TRANsform:DISTance:PVELocity <propagation-velocity>
> :CALCulate:TRANsform:DISTance:STARt <distance>{ m|cm|mm,ft}
> :CALCulate:TRANsform:DISTance:STOP <distance>{ m|cm|mm,ft}
> :CALCulate:TRANsform:DISTance:UNIT METers|FEET
> :CALCulate:TRANsform:DISTance:WINDow RECTangular|MSLobe|NSLobe|LSLobe
> :CAPTure:STARt
> :CAPTure:STOP
> :CAPTure:TRACe#:DATA? FDATa|SDATa|FMEM|SMEM
> :CONFigure:MEASure:DISPlay SINGle|DUAL
> :CONFigure:MEASure:MODe RLFReq|RLDTf|SWRFreq|SWRDtf|CLFReq|TRES|SMITh|PHASe
> :DISPlay:UPDate ON|OFF|1|0
> :DISPlay:WINDow:TRACe:STATe TRACe|MEMory|BOTH
> :DISPlay:WINDow:TRACe:Y[:SCALe]:AUToscale
> :DISPlay:WINDow:TRACe:Y[:SCALe]:BOTTom <amplitude>{dB}
> :DISPlay:WINDow:TRACe:Y[:SCALe]:FULLscale
> :DISPlay:WINDow:TRACe:Y[:SCALe]:TOP <amplitude>{dB}
> :FORMat[:READings][:DATA] ASCii|INTeger,32|REAL,32
> :FORMat[:READings][:DATA]:MULTiplier 1|1M
> :INITiate#:DATA? FDATa|SDATa|FMEM|SMEM
> :INITiate:CONTinuous OFF|ON|0|1
> :INITiate:HOLD OFF|ON|0|1
> :INITiate[:IMMediate]
> :SOURce:POWer LOW|HIGH
> [:SENSe]:CORRection:COLLect:ABORt
> [:SENSe]:CORRection:COLLect:INITialize
> [:SENSe]:CORRection:COLLect:LOAD
> [:SENSe]:CORRection:COLLect:OPEN
> [:SENSe]:CORRection:COLLect:SAVe
> [:SENSe]:CORRection:COLLect:SHORt
> [:SENSe]:CORRection:COLLect:THRU
> [:SENSe]:CORRection:COLLect:TYPE RFP1|2PES|TRES
> [:SENSe]:CORRection:COLLect:ZERO
> [:SENSe]:CORRection:INSTacal:CALibrate
> [:SENSe]:CORRection:TYPE STANdard|FLEX
> [:SENSe]:CORRection[:STATe] ON|OFF|1|0
> [:SENSe]:FREQuency:CABLe <cable-list-index>
> [:SENSe]:FREQuency:CABLe:NAMe <"cable-name">
> [:SENSe]:FREQuency:STARt <frequency>{ Hz|kHz|MHz|GHz}
> [:SENSe]:FREQuency:STOP <frequency>{ Hz|kHz|MHz|GHz}
> [:SENSe]:RFON[:STATe] ON|OFF|1|0
> [:SENSe]:SWEep:IFBW <frequency>{ Hz|kHz|MHz|GHz}
> [:SENSe]:SWEep:RESolution 130|259|517|1033|2065
> [:SENSe]:SWEep:RFIMmunity HIGH|LOW|1|0
> [:SENSe]:SWEep:TYPE CONTinuous|SINGle|EXTernal
> [:SENSe]:TRACe:SELect 1|2
> The commands in this section apply to the Cable and Antenna Analysis mode.
> :CALCulate#:DATA? FDATa|SDATa|FMEM|SMEM
> Query Description
> Query returns formatted data block of the specified trace.
> Param Range
> FDATa|SDATa|FMEM|SMEM
> Example
> To query trace 1 S-data:
> :CALC1:DATA? SDATA
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode. FDATa: Formatted (or Final) data. The returned data are based on the Measurement Mode that is associated with the trace. For measurement types that use only one number per point (such as Return Loss, VSWR, Cable Loss, Transmission, Phase), the command returns one number per data point. For graph types that use two numbers per point (such as Smith Chart), the command returns two numbers per data point. SDATa: Complex measurement data. The returned numbers, which are independent of the Measurement Mode that is associated with the trace, are complex measurement data pairs (Real and Imaginary) for each point of the trace. A 517 point trace therefore has a total of 1034 values that get transferred. FMEM: Formatted (or Final) Memory data. Similar to FDATa, but for memory data. SMEM: Complex memory data. Similar to SDATa, but for memory data. Note that in order to get valid data when querying for memory data, you must first store a trace into memory. The format of the block data that is returned can be specified by the command :FORMat[:READings][:DATA]. The response begins with an ASCII header that specifies the number of data bytes. It appears in the format #AX, where A is the number of digits in X, and X is the number of bytes that follow the header. Each data point is separated by a comma delimiter.
> :CALCulate#:LIMit:LOWer:SEGMent:ADD <StartX><StopX><StartY><StopY>
> Cmd Description
> Command adds a segment to the lower limit line.
> Param Type
> Float
> Default Units
> X units: Hz for Frequency domain, m or ft for Distance domain; Y units: same as current active trace y-axis units
> Example
> To add a lower limit segment from 1MHz to 1GHz with value 20 dB for trace 1:
> :CALC1:LIM:LOW:SEGM:ADD 1e6,1e9,20,20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer:SEGMent:DELete
> Cmd Description
> Command deletes the active lower segment.
> Example
> To delete the active lower segment for trace 1
> :CALC1:LIM:LOW:SEGM:DEL
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer:SEGMent:EDIT <StartX><StopX><StartY><StopY>
> Cmd Description
> Command edits the lower limit active segment. The active segment index must be updated when adding/deleting a segment.
> Param Type
> Float
> Default Units
> X units: Hz for Frequency domain, m or ft for Distance domain; Y units: same as current active trace y-axis units
> Example
> To edit the active segment and set it to 1MHz to 1GHz with value 20 dB for trace 1:
> :CALC1:LIM:LOW:SEGM:EDIT 1e6,1e9,20,20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer:SEGMent:STARt:X <value>
> :CALCulate#:LIMit:LOWer:SEGMent:STARt:X?
> Cmd Description
> Command sets the lower limit line X start value for current segment.
> Query Description
> Query returns the lower limit line X start value for active segment.
> Param Type
> Float
> Default Units
> Hz for Frequency domain, m or ft for Distance domain.
> Example
> To set limit X start value to 1 MHz for trace 1:
> :CALC1:LIM:LOW:SEGM:STAR:X 1000000
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer:SEGMent:STARt:Y <amplitude>
> :CALCulate#:LIMit:LOWer:SEGMent:STARt:Y?
> Cmd Description
> Command sets the lower limit line Y start value for active segment.
> Query Description
> Query returns the lower limit line Y start value for active segment.
> Param Type
> Float
> Default Units
> Current active trace y-axis units
> Example
> To set limit start amplitude to 20 dB for trace 1:
> :CALC1:LIM:LOW:SEGM:STAR:Y 20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer:SEGMent:STOP:X <value>
> :CALCulate#:LIMit:LOWer:SEGMent:STOP:X?
> Cmd Description
> Command sets the lower limit line X stop value for active segment.
> Query Description
> Query returns the upper limit line X stop value for active segment.
> Param Type
> Float
> Default Units
> Hz for Frequency domain, m or ft for Distance domain.
> Example
> To set limit X stop value to 1 MHz for trace 1:
> :CALC1:LIM:LOW:SEGM:STOP:X 1000000
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer:SEGMent:STOP:Y <amplitude>
> :CALCulate#:LIMit:LOWer:SEGMent:STOP:Y?
> Cmd Description
> Command sets the lower limit line Y stop value for active segment.
> Query Description
> Query returns the lower limit line Y stop value for active segment.
> Param Type
> Float
> Default Units
> Current active trace y-axis units
> Example
> To set limit stop amplitude to 20 dB for trace 1:
> :CALC1:LIM:LOW:SEGM:STOP:Y 20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer:SEGMent:TOTal?
> Query Description
> Query returns the total segments in the lower limit for the given trace.
> Example
> To query how many lower limit segments are currently available for trace 1:
> :CALC:LIM:LOW:SEGM:TOT?
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer:Y <amplitude>{dB,s|ms|ns|ps}
> :CALCulate#:LIMit:LOWer:Y?
> Cmd Description
> Command sets the lower limit line value. In group delay mode, the value is in units of time.
> Query Description
> Query returns the lower limit line value.
> Param Range
> x[,dB]
> Default Units
> Current active trace y-axis units
> Example
> To set limit amplitude to 20 dB for trace 1:
> :CALC1:LIM:LOW:Y 20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:LOWer[:STATe] OFF|ON|0|1
> :CALCulate#:LIMit:LOWer[:STATe]?
> Cmd Description
> Command sets the low limit line state for the specified trace.
> Query Description
> Query returns the lower limit line state for the specified trace.
> Param Range
> OFF|ON|0|1
> Default Value
> OFF|0
> Example
> To set limit on for trace 1:
> :CALC1:LIM:LOW ON
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:SEGMent:ADD <StartX><StopX><StartY><StopY>
> Cmd Description
> Command adds a segment to the upper limit line.
> Param Type
> Float
> Default Units
> X units: Hz for Frequency domain, m or ft for Distance domain; Y units: same as current active trace y-axis units
> Example
> To add an upper limit segment from 1MHz to 1GHz with value 20 dB for trace 1:
> :CALC1:LIM:UPP:SEGM:ADD 1e6,1e9,20,20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:SEGMent:DELete
> Cmd Description
> Command deletes the active upper segment.
> Example
> To delete the active upper segment for trace 1
> :CALC1:LIM:UPP:SEGM:DEL
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:SEGMent:EDIT <StartX><StopX><StartY><StopY>
> Cmd Description
> Command edits the upper limit active segment. The active segment index must be updated when adding/deleting a segment.
> Param Type
> Float
> Default Units
> X units: Hz for Frequency domain, m or ft for Distance domain; Y units: same as current active trace y-axis units
> Example
> To edit the active segment and set it to 1MHz to 1GHz with value 20 dB for trace 1:
> :CALC1:LIM:UPP:SEGM:EDIT 1e6,1e9,20,20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:SEGMent:STARt:X <value>
> :CALCulate#:LIMit:UPPer:SEGMent:STARt:X?
> Cmd Description
> Command sets the upper limit line X start value for active segment.
> Query Description
> Query returns the upper limit line X start value for active segment.
> Param Type
> Float
> Default Units
> Hz for Frequency domain, m or ft for Distance domain.
> Example
> To set limit X start value to 1 MHz for trace 1:
> :CALC1:LIM:UPP:SEGM:STAR:X 1000000
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:SEGMent:STARt:Y <amplitude>
> :CALCulate#:LIMit:UPPer:SEGMent:STARt:Y?
> Cmd Description
> Command sets the upper limit line Y start value for active segment.
> Query Description
> Query returns the upper limit line Y start value for active segment.
> Param Type
> Float
> Default Units
> Current active trace y-axis units
> Example
> To set limit start amplitude to 20 dB for trace 1:
> :CALC1:LIM:UPP:SEGM:STAR:Y 20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:SEGMent:STOP:X <value>
> :CALCulate#:LIMit:UPPer:SEGMent:STOP:X?
> Cmd Description
> Command sets the upper limit line X stop value for active segment.
> Query Description
> Query returns the upper limit line X stop value for active segment.
> Param Type
> Float
> Default Units
> Hz for Frequency domain, m or ft for Distance domain.
> Example
> To set limit X stop value to 1 MHz for trace 1:
> :CALC1:LIM:UPP:SEGM:STOP:X 1000000
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:SEGMent:STOP:Y <amplitude>
> :CALCulate#:LIMit:UPPer:SEGMent:STOP:Y?
> Cmd Description
> Command sets the upper limit line Y stop value for active segment.
> Query Description
> Query returns the upper limit line Y stop value for active segment.
> Param Type
> Float
> Default Units
> Current active trace y-axis units
> Example
> To set limit stop amplitude to 20 dB for trace 1:
> :CALC1:LIM:UPP:SEGM:STOP:Y 20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:SEGMent:TOTal?
> Query Description
> Query returns the total segments in the upper limit for the given trace.
> Example
> To query how many upper limit segments are currently available for trace 1:
> :CALC:LIM:UPP:SEGM:TOT?
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer:Y <amplitude>{dB,s|ms|ns|ps}
> :CALCulate#:LIMit:UPPer:Y?
> Cmd Description
> Command sets the upper limit line value. In group delay mode, the value is in units of time.
> Query Description
> Query returns the upper limit line value.
> Param Type
> Float
> Default Units
> Current active trace y-axis units
> Example
> To set limit amplitude to 20 dB for trace 1:
> :CALC1:LIM:UPP:Y 20
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate#:LIMit:UPPer[:STATe] OFF|ON|0|1
> :CALCulate#:LIMit:UPPer[:STATe]?
> Cmd Description
> Command sets the upper limit line state for the specified trace.
> Query Description
> Query returns the upper limit line state for the specified trace.
> Param Range
> OFF|ON|0|1
> Default Value
> OFF|0
> Example
> To set limit on for trace 1:
> :CALC1:LIM:UPP ON
> Notes
> Replace ’#’ with the required trace number. Check User Guide for the number of supported traces in each mode.
> :CALCulate:LIMit:ALARm OFF|ON|0|1
> :CALCulate:LIMit:ALARm?
> Cmd Description
> Command sets the limit alarm state. The device beeps if a trace point crosses the limit line.
> Query Description
> Query returns the limit alarm state.
> Param Range
> OFF|ON|0|1
> Default Value
> OFF|0
> Example
> To set limit alarm on:
> :CALC:LIM:ALAR ON
> :CALCulate:LIMit:LOWer:SEGMent:ACTive <Index>
> Cmd Description
> Command sets the given lower segment index active.
> Param Type
> int
> Example
> To set lower segment 1 active:
> :CALC:LIM:LOW:SEGM:ACT 1
> :CALCulate:LIMit:MESSage OFF|ON|0|1
> :CALCulate:LIMit:MESSage?
> Cmd Description
> Command sets the limit message state. Displays a Pass/Fail message to indicate whether the trace crosses the limit line.
> Query Description
> Query returns the limit message state.
> Param Range
> OFF|ON|0|1
> Default Value
> OFF|0
> Example
> To set limit message on:
> :CALC:LIM:MESS ON
> :CALCulate:LIMit:MESSage:RESult?
> Query Description
> Query returns 0 if limit line says Fail. Otherwise, it returns 1 if limit line says Pass.
> Example
> To get limit line Pass/Fail result:
> :CALC:LIM:MESS:RES?
> :CALCulate:LIMit:MODe
> Cmd Description
> Command changes the limit line to either Line or Segmented mode.
> Example
> To change the limit line mode
> :CALC:LIM:MOD SEGM
> :CALCulate:LIMit:PRESet
> Cmd Description
> Command presets the limit line to its default state.
> Example
> To perform limit line preset:
> :CALC:LIM:PRES
> :CALCulate:LIMit:TYPE 0|1
> :CALCulate:LIMit:TYPE?
> Cmd Description
> Command sets the active limit line type. 0 for upper limit and 1 for lower limit.
> Query Description
> Query returns the active limit line type.
> Param Range
> 0|1
> Default Value
> 0
> Example
> To set the active limit to lower limit:
> :CALC:LIM:TYPE 1
> :CALCulate:LIMit:UPPer:SEGMent:ACTive <Index>
> Cmd Description
> Command sets the given upper segment index active.
> Param Type
> int
> Example
> To set upper segment 1 active:
> :CALC:LIM:UPP:SEGM:ACT 1
> :CALCulate:LIMit:VALue <amplitude>{dB}
> :CALCulate:LIMit:VALue?
> Cmd Description
> Command sets the limit line value.
> Query Description
> Query returns the limit line value.
> Param Type
> Float
> Default Units
> Current active trace y-axis units
> Example
> To set limit line to 20 dB:
> :CALC:LIM:VAL 20
> :CALCulate:LIMit[:STATe] OFF|ON|0|1
> :CALCulate:LIMit[:STATe]?
> Cmd Description
> Command sets the limit line state.
> Query Description
> Query returns the limit line state.
> Param Range
> OFF|ON|0|1
> Default Value
> OFF|0
> Example
> To set limit on:
> :CALC:LIM ON
> :CALCulate:MARKer#:PEAK
> Cmd Description
> This command sets specified marker to the trace peak value.
> Example
> To set marker 5 to the peak of the trace:
> :CALC:MARK5:PEAK
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode.
> :CALCulate:MARKer#:PEAK:BOUNded
> Cmd Description
> This command sets specified marker to the trace peak value between two markers. Markers 5 and 7 will search for the peak between markers 1 and 2. Markers 6 and 8 will search for the peak between markers 3 and 4.
> Example
> To set marker 5 to the peak between markers 1 and 2:
> :CALC:MARK5:PEAK:BOUN
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode. If any marker other than 5, 6, 7, or 8 is specified, the bounded marker will be set to 5 by default.
> :CALCulate:MARKer#:TRACking PEAK|VALLey|BNDPeak|BNDValley|OFF
> :CALCulate:MARKer#:TRACking?
> Cmd Description
> Command sets the tracking mode of the specified marker.
> Query Description
> Query returns the tracking mode of the specified marker. Query returns PEAK for peak tracking, or returns VALL for valley tracking, or returns BNDP for bounded peak tracking, or returns BNDV for bounded valley tracking.
> Param Range
> PEAK|VALLey|BNDPeak|BNDValley|OFF
> Default Value
> OFF
> Example
> To set marker 2 to peak tracking:
> :CALC:MARK2:TRAC PEAK
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode. If any marker other than 5, 6, 7, or 8 is specified, the bounded marker will be set to 5 by default.
> :CALCulate:MARKer#:TYPE REFerence|DELTa
> :CALCulate:MARKer#:TYPE?
> Cmd Description
> Command sets the type of the specified marker.
> Query Description
> Query returns the type of the specified marker. Query returns REF if the specified marker is a reference marker, or returns DELT if the specified marker is a delta marker.
> Param Range
> REFerence|DELTA
> Default Value
> REF
> Example
> To set marker 2 type to delta:
> :CALC:MARK2:TYPE DELT
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode.
> :CALCulate:MARKer#:VALLey
> Cmd Description
> This command sets specified marker to the trace valley value.
> Example
> To set marker 5 to the valley of the trace:
> :CALC:MARK5:VALL
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode.
> :CALCulate:MARKer#:VALLey:BOUNded
> Cmd Description
> This command sets specified marker to the trace valley value between two markers. Markers 5 and 7 will search for the valley between markers 1 and 2. Markers 6 and 8 will search for the valley between markers 3 and 4.
> Example
> To set marker 5 to the valley between markers 1 and 2:
> :CALC:MARK5:VALL:BOUN
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode. If any marker other than 5, 6, 7, or 8 is specified, the bounded marker will be set to 5 by default.
> :CALCulate:MARKer#:X <value>{Hz|kHz|MHz|GHz,m|cm|mm,ft}
> :CALCulate:MARKer#:X?
> Cmd Description
> Command sets the position for the specified marker in the current sweep domain. For delta marker, it sets the relative position to the reference marker. Verify that the appropriate unit is used.
> Query Description
> Query returns the marker position for the specified marker. For a delta marker, query returns the position relative to the reference marker.
> Param Type
> Float
> Param Description
> Frequency, or distance.
> Default Value
> Model-dependent
> Default Units
> Hz
> Example
> To set marker 2 frequency to 1 GHz:
> :CALC:MARK2:X 1 GHZ
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode.
> :CALCulate:MARKer#:Y?
> Query Description
> Query returns the amplitude value for the specified marker.
> Example
> To query marker 3 amplitude value:
> :CALC:MARK3:Y?
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode.
> :CALCulate:MARKer#[:STATe] OFF|ON|0|1
> :CALCulate:MARKer#[:STATe]?
> Cmd Description
> Command sets the state of the specified marker.
> Query Description
> Query returns the state of the specified marker. Query returns 1 if the specified marker is on, or returns 0 if the specified marker is off.
> Param Range
> OFF|ON|0|1
> Default Value
> OFF|0
> Example
> To set marker 1 state ON:
> :CALC:MARK1 ON
> Notes
> Replace ’#’ with the required marker number. Check User Guide for the number of supported markers in each mode.
> :CALCulate:MARKer:ACTive?
> Query Description
> Query returns active marker number. Returns NONE if no markers are active.
> Example
> To get active marker
> :CALC:MARK:ACT?
> :CALCulate:MARKer:DISPlay MKRTable|MKRonly|AOFF
> :CALCulate:MARKer:DISPlay?
> Cmd Description
> Command sets the marker display mode.
> Query Description
> Query returns the marker display mode. Query returns MKRT if the markers and marker table are displayed, returns MKR if only the markers are displayed, or returns AOFF if markers and marker table are not displayed.
> Param Range
> MKRTable|MKRonly|AOFF
> Default Value
> MKRTable
> Example
> To set marker display to marker only:
> :CALC:MARK:DISP MKR
> :CALCulate:MARKer:PRESet
> Cmd Description
> Presets markers.
> Example
> To preset markers:
> :CALC:MARK:PRES
> :CALCulate:MATH:FUNCtion NONE|SUBTraction|ADDition|AVERage
> :CALCulate:MATH:FUNCtion?
> Cmd Description
> Command sets the trace math function. NONE - no trace math applied; SUBT - memory trace subtracted from active trace; ADD - memory trace added to active trace; AVER - active and memory traces added and divided by 2.
> Query Description
> Query returns the trace math function.
> Param Range
> NONE|SUBTraction|ADDition|AVERage
> Default Value
> NONE
> Example
> To set trace math function to addition:
> :CALC:MATH:FUNC ADD
> :CALCulate:MATH:MEMorize
> Cmd Description
> Copies active trace into the memory buffer.
> Example
> To copy active trace into the memory buffer:
> :CALC:MATH:MEM
> :CALCulate:TRANsform:CLAVerage?
> Query Description
> Query returns cable loss average when the measurement mode is ’Cable Loss’.
> Default Units
> dB
> Example
> To query cable loss average:
> :CALC:TRAN:CLAV?
> :CALCulate:TRANsform:DISTance:CABLoss <cable-loss>{ dB/m,dB/ft}
> :CALCulate:TRANsform:DISTance:CABLoss?
> Cmd Description
> Command sets the cable loss. Verify that the appropriate unit is used.
> Query Description
> Query returns the cable loss based on the current units.
> Param Type
> Float
> Default Value
> 0
> Default Units
> dB/m
> Example
> To set cable loss to 2:
> :CALC:TRAN:DIST:CABL 2
> :CALCulate:TRANsform:DISTance:DMAX?
> Query Description
> Query returns max distance in the current units.
> Example
> To query max distance:
> :CALC:TRAN:DIST:DMAX?
> :CALCulate:TRANsform:DISTance:PVELocity <propagation-velocity>
> :CALCulate:TRANsform:DISTance:PVELocity?
> Cmd Description
> Command sets the propagation velocity.
> Query Description
> Query returns the propagation velocity.
> Param Type
> Float
> Default Value
> 1
> Example
> To set propagation velocity to 0.05:
> :CALC:TRAN:DIST:PVEL 0.05
> :CALCulate:TRANsform:DISTance:RESolution?
> Query Description
> Query returns distance resolution in the current units for reflection.
> Example
> To query distance resolution:
> :CALC:TRAN:DIST:RESolution?
> :CALCulate:TRANsform:DISTance:STARt <distance>{ m|cm|mm,ft}
> :CALCulate:TRANsform:DISTance:STARt?
> Cmd Description
> Command sets the start distance. Verify the appropriate unit is used.
> Query Description
> Query returns the start distance in the current units.
> Param Type
> Float
> Param Description
> Distance
> Default Units
> m(meter)
> Example
> To set start distance to 1 m:
> :CALC:TRAN:DIST:STAR 1
> :CALCulate:TRANsform:DISTance:STOP <distance>{ m|cm|mm,ft}
> :CALCulate:TRANsform:DISTance:STOP?
> Cmd Description
> Command sets the stop distance. Verify the appropriate unit is used.
> Query Description
> Query returns the stop distance in the current units.
> Param Type
> Float
> Param Description
> Distance
> Default Units
> m(meter)
> Example
> To set stop distance to 2 m:
> :CALC:TRAN:DIST:STOP 2 M
> :CALCulate:TRANsform:DISTance:UNIT METers|FEET
> :CALCulate:TRANsform:DISTance:UNIT?
> Cmd Description
> Command sets the distance unit.
> Query Description
> Query returns the current distance units.
> Param Range
> METers|FEET
> Default Value
> METers
> Example
> To set distance unit to feet:
> :CALC:TRAN:DIST:UNIT FEET
> :CALCulate:TRANsform:DISTance:WINDow RECTangular|MSLobe|NSLobe|LSLobe
> :CALCulate:TRANsform:DISTance:WINDow?
> Cmd Description
> Command sets the window type for distance domain.
> Query Description
> Query returns the window type for distance domain.
> Param Type
> Character
> Param Range
> RECTangular|MSLobe|NSLobe|LSLobe
> Default Value
> NSLobe
> Example
> To set distance domain window type to rectangular:
> :CALC:TRAN:DIST:WIND RECT
> :CAPTure:STARt
> Cmd Description
> Command starts the data capture for continuous sweeps. It does not work in single sweep and hold mode.
> Example
> To start data capture
> :CAPT:STAR
> :CAPTure:STOP
> Cmd Description
> Command stops the data capture for continuous sweeps. It does not work in single sweep and hold mode.
> Example
> To stop capture:
> :CAPT:STOP
> :CAPTure:TRACe#:DATA? FDATa|SDATa|FMEM|SMEM
> Cmd Description
> Command is used to return the data block of the specified trace at the end of a sweep, while the instrument is in continuous sweep mode. This command must follow the :CAPTure:STARt command. A :CAPTure:STOP command is used to end the capture session. If the system is in single sweep and hold mode, then this command is ignored.
> Example
> To trigger a sweep:
> :CAPT:TRAC1:DATA? FDAT
> :CONFigure:MEASure:DISPlay SINGle|DUAL
> :CONFigure:MEASure:DISPlay?
> Cmd Description
> Command sets the display format to single or dual traces. Only supported in Advanced Cable & Antenna Analyzer mode.
> Query Description
> Query returns the display format. Only supported in Advanced Cable & Antenna Analyzer mode.
> Param Range
> SINGle|DUAL
> Default Value
> SINGle
> Example
> To set display format to dual traces:
> :CONF:MEAS:DISP DUAL
> :CONFigure:MEASure:MODe RLFReq|RLDTf|SWRFreq|SWRDtf|CLFReq|TRES|SMITh|PHASe
> :CONFigure:MEASure:MODe?
> Cmd Description
> Command sets the active trace measurement mode.
> Query Description
> Query returns the current measurement mode.
> Param Description
> RLFReq: Return Loss(Frequency domain sweep); RLDTf: Return Loss(DTF); SWRFreq: SWR(Frequency domain sweep); SWRDtf: SWR(DTF); CLFReq: Cable Loss - One Port(Frequency domain sweep); TRES: Transmission - External Sensor; SMITh: Smith Chart; PHASe: One-Port Phase. TRES, SMITh, and PHASe are not available in Classic Mode.
> Example
> To set measurement mode to Cable Loss:
> :CONF:MEAS:MOD CLFR
> :DISPlay:UPDate ON|OFF|1|0
> :DISPlay:UPDate?
> Cmd Description
> Command sets the display update on/off.
> Query Description
> Query returns display update status. Query returns 1 if display update is on. Otherwise, it returns 0.
> Param Range
> ON|OFF|1|0
> Default Value
> OFF|0
> Example
> To turn display update off:
> :DISP:UPD OFF
> :DISPlay:WINDow:TRACe:STATe TRACe|MEMory|BOTH
> :DISPlay:WINDow:TRACe:STATe?
> Cmd Description
> Command sets the trace display type for the active trace. TRAC - only active trace is shown; MEM - only memory trace is shown; BOTH - both active and memory traces are shown. Use :CALCulate:MATH:MEMorize before changing the display type.
> Query Description
> Query returns the trace display type.
> Param Range
> TRACe|MEMory|BOTH
> Default Value
> TRACe
> Example
> To show both active and memory trace on the display:
> :DISP:WIND:TRAC:STAT BOTH
> :DISPlay:WINDow:TRACe:Y[:SCALe]:AUToscale
> Cmd Description
> This command sets the top and bottom values such that the trace occupies a significant portion of the grid.
> Example
> To perform auto-scale:
> :DISP:WIND:TRAC:Y:AUT
> :DISPlay:WINDow:TRACe:Y[:SCALe]:BOTTom <amplitude>{dB}
> :DISPlay:WINDow:TRACe:Y[:SCALe]:BOTTom?
> Cmd Description
> Command sets the display bottom value.
> Query Description
> Query returns the display bottom value.
> Param Type
> Float
> Default Value
> Return Loss = 60dB; DTF Return Loss = 60dB; Cable Loss = 30dB; VSWR = 1; DTF VSWR = 1; Transmission = -90dB; Phase=-225
> Default Units
> dB
> Example
> To set trace bottom value in Return Loss to 40 dB:
> :DISP:WIND:TRAC:Y:BOTT 40
> :DISPlay:WINDow:TRACe:Y[:SCALe]:FULLscale
> Cmd Description
> Sets the top and bottom to their maximum values.
> Example
> To perform full-scale:
> :DISP:WIND:TRAC:Y:FULL
> :DISPlay:WINDow:TRACe:Y[:SCALe]:TOP <amplitude>{dB}
> :DISPlay:WINDow:TRACe:Y[:SCALe]:TOP?
> Cmd Description
> Command sets the display top value.
> Query Description
> Query returns the display top value.
> Param Type
> Float
> Default Value
> Return Loss = 0dB; DTF Return Loss = 0dB; Cable Loss = 0dB; VSWR = 3; DTF VSWR = 3; Transmission = 10dB; Phase = 225
> Default Units
> dB
> Example
> To set trace top value in Return Loss to 10 dB:
> :DISP:WIND:TRAC:Y:TOP 10
> :FORMat[:READings][:DATA] ASCii|INTeger,32|REAL,32
> :FORMat[:READings][:DATA]?
> Cmd Description
> Command sets the data format type. ASCii and REAL returns data in current unit. INTeger returns data with mdBm unit. This command applies to :TRACe[:DATA]? and :CALCulate:DATA?.
> Query Description
> Query returns the data format type as ASC or INT, 32 or REAL, 32.
> Param Range
> ASCii|INTeger,32|REAL,32
> Example
> To set data format type to integer:
> :FORM INT,32
> Notes
> INTeger,32 values are signed 32-bit integers in little-endian byte order. This format returns the data in 4-byte blocks. REAL,32 values are 32-bit floating point numbers conforming to the IEEE 754 standard in little-endian byte order. This format returns the data in 4-byte binary format. The units are the current instrument units. Both INTeger and REAL formats return a definite block length. Each transfer begins with an ASCII header, such as #42204 for INTeger,32 and REAL,32. The first digit represents the number of following digits in the header.
> :FORMat[:READings][:DATA]:MULTiplier 1|1M
> :FORMat[:READings][:DATA]:MULTiplier?
> Cmd Description
> Command sets the data format multiplier factor.
> Query Description
> Query returns the data format multiplier factor. If ’1M’ is passed as argument, then query results for :TRACe[:DATA]? and :CALCulate:DATA? will specify readings multiplied by 10^6. If ’1’ is passed, then query results for :TRACe[:DATA]? and :CALCulate:DATA? will specify read.
> Param Range
> 1|1M
> Default Value
> 1M
> Example
> To set data format multiplier to 1:
> :FORM:MULT 1
> :INITiate#:DATA? FDATa|SDATa|FMEM|SMEM
> Cmd Description
> Command triggers a sweep and returns the data block of the specified trace at the end of sweep. If the system is in continuous mode, then this command is ignored.
> Example
> To trigger a sweep and wait for Formatted data to be returned:
> :INIT1:DATA? FDAT
> :INITiate:CONTinuous OFF|ON|0|1
> :INITiate:CONTinuous?
> Cmd Description
> Command sets the sweep type between single sweep and continuous sweep.
> Query Description
> Query returns the sweep type, single or continuous. Query returns 1 for continuous sweep, and returns 0 for single sweep.
> Param Range
> OFF|ON|0|1
> Default Value
> ON|1
> Example
> To set the sweep type to single sweep:
> :INIT:CONT OFF
> :INITiate:HOLD OFF|ON|0|1
> :INITiate:HOLD?
> Cmd Description
> Command sets the sweep state between run and hold. This command is ignored in external trigger mode.
> Query Description
> Query returns the sweep state, run or hold. Query returns 1 for hold mode, and returns 0 for run mode.
> Param Range
> OFF|ON|0|1
> Default Value
> OFF|0
> Example
> To set the sweep state to hold:
> :INIT:HOLD ON
> :INITiate[:IMMediate]
> Cmd Description
> Command triggers a single sweep if in single sweep mode. If the system is in continuous mode, then this command is ignored.
> Example
> To trigger a sweep:
> :INIT
> :SOURce:POWer LOW|HIGH
> :SOURce:POWer?
> Cmd Description
> Command sets the source power level. Default is high.
> Query Description
> Query returns the source power level, LOW or HIGH.
> Example
> To set source power to low:
> SOUR:POW LOW
> :STATus:OPERation?
> Query Description
> Queries sweep status. This is used in combination with :INITiate[:IMMediate]. Sweep complete bit is the bit 8. Query returns 256 if sweep has completed. Otherwise, it returns 0.
> Example
> To query sweep status:
> :STAT:OPER?
> :TRACe[:DATA]? {1|2}
> Query Description
> Query returns raw trace data in real and imaginary format.
> Param Type
> Integer
> Param Description
> Optional Param: Trace number, default is 1.
> Param Range
> 1|2
> Example
> To get trace 1 data:
> :TRAC?
> Notes
> The format of the block data that is returned can be specified by the command :FORMat[:READings][:DATA]. The response begins with an ASCII header that specifies the number of data bytes. It appears in the format #AX, where A is the number of digits in X, and X is the number of bytes that follow the header. Each data point is separated by a comma-delimiter. The returned numbers, which are independent of the Measurement Mode that is associated with the trace, are complex measurement data pairs (Real and Imaginary) for each point of the trace. A 517 point trace therefore has a total of 1034 values that get transferred.
> [:SENSe]:APPLication:TST:RESult?
> Query Description
> Query returns self-test details. The self-test command (See [:SENSe]:APPLication:TST? [NORMal]) must be sent before getting the self-test details.
> Example
> To retrieve application self-test result:
> :APPL:TST:RES?
> Notes
> The response begins with an ASCII header. The header specifies the number of following bytes. It appears in the format #AX, where A is the number of digits in X, and X is the number of bytes that follow the header. The first information of the result contains the overall self test string ("PASSED" or "FAILED") followed by a comma, and each self-test result separated by a comma. Each subset of the result is included in angled brackets.
> [:SENSe]:APPLication:TST? {NORMal}
> Query Description
> Query returns 0 if self-test succeeds with no error. Otherwise, it returns 255.
> Param Description
> Optional Param: Self-test type, default is NORMal.
> Param Range
> NORMal
> Example
> To run an application self-test:
> :APPL:TST?
> [:SENSe]:CALibration:STATe?
> Query Description
> Query returns the state of calibrated measurements depending on the calibration collection type. 0 means no calibration was done. For calibration type RFP1 (OSL), return value is 1. For calibration type TRES (Transmission w/External Sensor), return value is 4. For calibration types 2PES (OSL + Transmission w/External Sensor), return value is 5.
> Example
> To query state after calibration is completed:
> :CAL:STAT?
> [:SENSe]:CORRection:COLLect:ABORt
> Cmd Description
> Aborts all steps of the RF calibration.
> Example
> To abort RF calibration:
> :CORR:COLL:ABOR
> [:SENSe]:CORRection:COLLect:INFO:STATus?
> Query Description
> Query returns 0 if calibration is not in progress, 1 if calibration is in progress, 2 if calibration was aborted, 3 if cal-coefficients are being calculated, or 4 if calibration has completed.
> Example
> To query calibration progress status:
> :CORR:COLL:INFO:STAT?
> [:SENSe]:CORRection:COLLect:INITialize
> Cmd Description
> Command to initialize an RF calibration with the current calibration type.
> Example
> To initialize RF calibration:
> :CORR:COLL:INIT
> [:SENSe]:CORRection:COLLect:LOAD
> Cmd Description
> Perform ’Load’ step of calibration.
> Example
> To measure load:
> :CORR:COLL:LOAD
> [:SENSe]:CORRection:COLLect:OPEN
> Cmd Description
> Perform ’Open’ step of calibration.
> Example
> To measure open:
> :CORR:COLL:OPEN
> [:SENSe]:CORRection:COLLect:SAVe
> Cmd Description
> Complete an RF Cal and perform coefficient calculation.
> Example
> To complete a RF calibration and perform coefficient calculation:
> :CORR:COLL:SAV
> [:SENSe]:CORRection:COLLect:SHORt
> Cmd Description
> Perform ’Short’ step of calibration.
> Example
> To measure short:
> :CORR:COLL:SHOR
> [:SENSe]:CORRection:COLLect:STATus? INITialize|OPEN|SHORt|LOAD|SAVE|ALL|THRU|ZERO
> Query Description
> Query returns 1 if a specified cal step is completed. Otherwise, it returns 0.
> Param Range
> INITialize|OPEN|SHORt|LOAD|SAVE|ALL|THRU|ZERO
> Example
> To query calibration step ’Open’ status:
> :CORR:COLL:STAT? OPEN
> [:SENSe]:CORRection:COLLect:THRU
> Cmd Description
> Perform ’Thru’ step of calibration.
> Example
> To measure Thru:
> :CORR:COLL:THRU
> [:SENSe]:CORRection:COLLect:TYPE RFP1|2PES|TRES
> [:SENSe]:CORRection:COLLect:TYPE?
> Cmd Description
> Command sets calibration collection type.
> Query Description
> Query returns calibration collection type.
> Param Range
> RFP1|2PES|TRES, Classic Cable & Antenna Analyzer Mode only supports RFP1
> Default Value
> RFP1
> Example
> To set collection type to RFP1:
> :CORR:COLL:TYPE RFP1
> [:SENSe]:CORRection:COLLect:ZERO
> Cmd Description
> Perform ’Zero Sensor’ step of calibration.
> Example
> To zero sensor:
> :CORR:COLL:ZERO
> [:SENSe]:CORRection:INSTacal:CALibrate
> Cmd Description
> Performs InstaCal.
> Example
> To perform a InstaCal:
> :CORR:INST:CAL
> [:SENSe]:CORRection:TYPE STANdard|FLEX
> [:SENSe]:CORRection:TYPE?
> Cmd Description
> Command sets correction type.
> Query Description
> Query returns correction type. Query returns STAN|FLEX.
> Param Range
> STANdard|FLEX
> Default Value
> STANdard
> Example
> To set correction type to flex:
> :CORR:TYPE FLEX
> [:SENSe]:CORRection[:STATe] ON|OFF|1|0
> [:SENSe]:CORRection[:STATe]?
> Cmd Description
> Command sets correction status.
> Query Description
> Query returns correction status. Query returns 1 if RF cal is on. Otherwise, it returns 0.
> Param Range
> ON|OFF|1|0
> Default Value
> OFF|0
> Example
> To turn calibration correction on:
> :CORR:STAT ON
> [:SENSe]:FREQuency:CABLe <cable-list-index>
> [:SENSe]:FREQuency:CABLe?
> Cmd Description
> Command selects a cable with the index number from the sorted cable list.
> Query Description
> Query returns the index number of the selected cable based on the sorted cable list.
> Param Type
> Integer
> Param Description
> Index number from cable list
> Default Value
> 0
> Example
> To set the cable index to 10:
> :FREQ:CABL 10
> [:SENSe]:FREQuency:CABLe:CATalog:FULL?
> Query Description
> Query returns the entire cable list that is stored in memory.
> Example
> To get the cable list:
> :FREQ:CABL:CAT:FULL?
> [:SENSe]:FREQuency:CABLe:NAMe <"cable-name">
> [:SENSe]:FREQuency:CABLe:NAMe?
> Cmd Description
> Command sets the cable name.
> Query Description
> Query returns the cable name.
> Param Type
> String
> Param Description
> Cable name
> Default Value
> NONE
> Example
> To set the cable to "AVA5-50 7/8":
> :FREQ:CABL:NAM "AVA5-50 7/8"
> [:SENSe]:FREQuency:STARt <frequency>{ Hz|kHz|MHz|GHz}
> [:SENSe]:FREQuency:STARt?
> Cmd Description
> Command sets the start frequency.
> Query Description
> Query returns the start frequency in Hertz.
> Param Type
> Float
> Param Description
> Start frequency
> Default Value
> Model-dependent
> Default Units
> Hz
> Example
> To set the start frequency to 2 GHz:
> :FREQ:STAR 2 GHZ
> [:SENSe]:FREQuency:STOP <frequency>{ Hz|kHz|MHz|GHz}
> [:SENSe]:FREQuency:STOP?
> Cmd Description
> Command sets the stop frequency.
> Query Description
> Query returns the stop frequency in Hertz.
> Param Type
> Float
> Param Description
> Stop frequency
> Default Value
> Model-dependent
> Default Units
> Hz
> Example
> To set the stop frequency to 2 GHz:
> :FREQ:STOP 2 GHZ
> [:SENSe]:RFON[:STATe] ON|OFF|1|0
> [:SENSe]:RFON[:STATe]?
> Cmd Description
> Command sets the RF power output state when the sweep is in Hold mode.
> Query Description
> Query returns the RF power output state when the sweep is in Hold mode.
> Param Range
> ON|OFF|1|0
> Default Value
> ON|1
> Example
> To set RF power output state off:
> :RFON OFF
> [:SENSe]:ROSCillator[:SOURce]?
> Query Description
> Query returns reference oscillator setting. Query returns INT for internal or EXT for external.
> Example
> To query reference oscillator:
> :ROSC?
> [:SENSe]:SWEep:IFBW <frequency>{ Hz|kHz|MHz|GHz}
> [:SENSe]:SWEep:IFBW?
> Cmd Description
> Command sets the IF bandwidth. The permissible values are 10Hz, 100Hz, 1kHz, 2kHz, and 100kHz.
> Query Description
> Query returns the IF bandwidth.
> Param Type
> Float
> Param Description
> Bandwidth frequency
> Default Units
> Hz
> Example
> To set IFBW to 1000Hz:
> :SWE:IFBW 1 kHz
> [:SENSe]:SWEep:RESolution 130|259|517|1033|2065
> [:SENSe]:SWEep:RESolution?
> Cmd Description
> Command sets the data points.
> Query Description
> Query returns the data points as a number.
> Param Range
> 130|259|517|1033|2065
> Default Value
> 259
> Example
> To set data points to 1033:
> :SWE:RES 1033
> [:SENSe]:SWEep:RFIMmunity HIGH|LOW|1|0
> [:SENSe]:SWEep:RFIMmunity?
> Cmd Description
> Command sets the RF immunity state.
> Query Description
> Query returns the RF immunity state, 1 for low immunity and 0 for high immunity.
> Param Range
> HIGH|LOW|1|0
> Default Value
> LOW|1
> Example
> To set RF immunity to low:
> :SWE:RFIM LOW
> [:SENSe]:SWEep:TYPE CONTinuous|SINGle|EXTernal
> Cmd Description
> Command sets the sweep trigger type to be Internal (Continuous or Single) or External.
> Param Range
> CONTinuous|SINGle|EXTernal
> Default Value
> CONTinuous
> Example
> To set the sweep trigger type to internal single sweep:
> :SWE:TYPE SING
> Notes
> External Trigger setting is not available on all models.
> [:SENSe]:TRACe:SELect 1|2
> [:SENSe]:TRACe:SELect?
> Cmd Description
> Command sets the active trace.
> Query Description
> Query returns the active trace.
> Param Range
> 1|2
> Default Value
> 1
> Example
> To set active trace to trace 2:
> :TRAC:SEL 2