> Amplitude Menu
> Key Sequence: Amplitude

> High Accuracy PM (MA24105A) Amplitude Menu

> Amplitude
> Max Value
> Sets the maximum value on the display in dBm or Watts.
> Min Value
> Sets the minimum value on the display in dBm or Watts.
> Autoscale
> Adjusts the Top and Bottom values so that the power meter needle will be shown in the middle of the analog display.
> Fullscale
> Adjusts the Top and Bottom values to their maximum allowed values (default settings). Offset Value
> Used to set external power attenuation or gain. The displayed power level is offset by the dB value entered.
> Offset Value
> Used to set external power attenuation or gain. The displayed power level is offset by the dB value entered.
> Units dBm Watts
> Sets the unit of measure for the power meter.
> Relative
> Fwd Relative On Off
> Press this submenu key to toggle On or Off. This measurement shows the relative level of the current forward power level to the forward power level when Fwd Relative was turned on.
> Rev Relative On Off
> Press this submenu key to toggle On or Off. This measurement shows the relative level of the current reverse power level to the reverse power level when Rev Relative was turned on.
> Note: The message Relative On shows in the message area when either Fwd or Rev Relative is on.