> Measurement Review
> Table: Cable and Antenna Measurement Overview provides a summary of the typical measurements and required cable end tool. The typical values are for general information purposes. The carriers will provide final values in the acceptance testing specification.

> Cable and Antenna Measurement Overview
> Measurement | Mode | End Tool | Marker
> TYPICAL PASS/FAIL MEASUREMENTS
> Pass/Fail Test of Cable & Connectors | Freq Return Loss or (Freq, SWR) | Load | Peak
> Pass/Fail Test of System Including Antenna | Freq Return Loss or (Freq, SWR) | Antenna | Peak
> Frequency Range of Antenna | Freq Return Loss or (Freq, SWR) | Antenna | Valley
> Cable Loss | Freq Cable Loss | Short or Open | Peak & Valley
> Cable Loss (High Accuracy) | Freq Cable Loss (Open and Short) / 2 using trace memory function | Short and Open | Peak
> Return Loss | Freq Return Loss | Load | Peak
> TROUBLESHOOTING MEASUREMENTS
> Cable Length | DTF Return Loss or (DTF SWR) | Short or Open | Peak
> Good Cable & Connectors | DTF Return Loss or (DTF SWR) | Load | Peak
> Good System Including Antenna | DTF Return Loss or (DTF SWR) | Antenna | Peak