> GPS Menu
> To use GPS, you must have an external USB-based GPS module connected.
> Key Sequence: System (8) > Connectivity > GPS

> GPS Menu

> Clear Data
> Press this key to clear the Site Master’s current GPS location data or last known GPS location data. If the 2000-1723-R or compatible GPS module is attached, the instrument will attempt to re-acquire a GPS fix.
> Note: The last Good Fix location information will be retained until the instrument is powered off, the Clear Data button is pressed, or a new Good Fix is acquired. The Good Fix or the Last Fix location information is stored in the measurement file and is included in the screen capture header/footer.
> Sync System Time
> Press this key to sync the instrument’s time setting with the current GPS information. Sync only works with a good GPS fix.
> After a valid sync, the instrument time is reset based on the UTC time plus/minus the time zone offset. Refer to Time Zone Settings.

> GPS Info

> Note | An exclamation mark (!) is appended to the GPS location data in screen captures when the instrument is using Last Fix instead of current GPS information.

> (!) Indicates Last Fix GPS Data