> Screen Shot Capture
> The Site Master can capture a bit mapped image of the display in Portable Network Graphics (.png) format using the ScrnShot (4) key or the Camera icon,.
> The file is automatically named based on the instrument model and measurement type. Screen shot files are saved to the instrument’s internal memory in the ScrnShots folder (Drive : Internal | ScrnShots).
> The look of the saved screen shot is set in this location: System (8) > System Setups > Display/Audio > ScrnShot Settings. Refer to the Display/Audio Menu for details. Figure: Screen Shot Settings is an example of the same measurement saved with different screen shot settings.

> Note | Measurements can also be saved as screen shots using the Save (7) menu, and then, setting the Filetype to ScreenShot. Using the Save menu allows the file name and location to be set by the user. Refer to File Management for additional information.

> Screen Shot Settings