> Amplitude
> Setting the Amplitude using Top and Bottom Keys

> 1. | Press the Amplitude main menu key.

> 2. | Press the Top submenu key and use the keypad, rotary knob, or the Up/Down arrow key to edit the top scale value. Press Enter to set.

> 3. | Press the Bottom key and use the keypad, rotary knob, or the Up/Down arrow key to edit the bottom scale value. Press Enter to set.

> Setting the Amplitude using Autoscale
> With Autoscale, the instrument will automatically set the top and bottom scales to display the current measurement.

> 1. | Press the Amplitude main menu key.

> 2. | Press the Autoscale submenu key.

> Setting the Amplitude using Fullscale
> With Fullscale, the instrument will automatically set the top and bottom scales to the default values based on the measurement type.

> 1. | Press the Amplitude main menu key.

> 2. | Press the Fullscale submenu key.

> Refer to Amplitude Menu for additional information.