> Sweep Menu
> Key Sequence: Sweep (3)

> Sweep Menu

> Data Points
> Sets the number of data points: 130, 259, 517, 1033 or 2065.
> Run/Hold
> Toggles between Run and Hold. When in Hold mode, pressing this key starts the sweeping and provides a trigger. When in the Run mode, pressing this key pauses the sweep.
> Sweep Type
> This toggles the sweep between single sweep and continuous sweep. In single sweep mode, each sweep must be activated by the Run/Hold key.
> RF Immunity, High / Low
> The instrument defaults to RF Immunity High and is the suggested setting. See RF Immunity for details.
> RF Pwr In Hold
> Sets the RF Output power to be turned off when Run/Hold is toggled to Hold. See RF Pwr In Hold for details.