> System Menu
> Key Sequence: System (8)

> System Menu (1 of 2)

> System Info
> Status
> Press this submenu key to display the Status Menu, which includes detailed instrument, hardware, software and connectivity information.
> Battery
> Press this key to display the battery charge remaining and charge status.
> System Setups
> Date/Time
> Press to display the Time and Date Menu.
> Language
> Press to set the default language. Options include: English, French, German, Italian, Spanish, Russian, Portuguese, Japanese, Korean, or Chinese.
> Display/Audio
> Press this submenu key to access the Display/Audio Menu, which includes display, screen shot, and volume settings.
> Connectivity
> GPS
> Press to display the GPS Menu.
> Ethernet Configuration
> Press this submenu key to display the Ethernet Configuration Menu, which shows the IP Address and MAC Address of the instrument and allows you to choose the setting for obtaining the IP Address (DHCP or Static).

> Diagnostics
> Self Test
> Press this submenu key to initiate a series of diagnostic tests that check the components of the instrument. A display lists the individual tests with a pass or fail indication ( Figure: Site Master Self Test). Press Esc to close the dialog box.
> Press Save to File to create a text file of the test results. The file is saved to internal memory and labeled S331LSelfTest#X.txt. The .txt file can be copied to a USB memory device and viewed on a PC with a text reader or word processor.