> Setup and Operation Summary

> 1. | Attach to the VIP a probe tip, or ferrule adapter, that is compatible with the type of fiber optic connector you wish to test. Refer to Connect the VIP.

> 2. | Connect the probe to the fiber optic endface and to the USB port on the Site Master S331L.

> 3. | On the Site Master, select VIP Mode. Refer to Launch the VIP Application. The instrument screen will display a live image of the fiber edge surface.

> 4. | Press the Setup main menu key and verify or change the VIP test settings, which include the probe model, tip type, and test profile. Refer to VIP Test Settings.

> 5. | If needed, use the Focus Control knob on the probe to adjust the image focus.

> 6. | Press the Measurement key on the Site Master screen, then press the Captured key to capture the displayed image.

> 7. | Turn the rotary knob to zoom the captured image. Use the arrow keys to pan.

> 8. | Press the Analyze key to execute analysis of the current VIP image. Detailed analysis results are displayed in tabular form if Auto is selected with the Results Table key.

> 9. | To quickly save the captured image and test results using the current auto filename settings, press the Save icon on the System Function Tool Bar. You can also press the Save/Recall main menu key, then press Save to manually enter a file name and select its location.

> 10. | Press Report if you wish to generate a report, in PDF format, on either the current or previously saved analysis results, or both.