> Cable and Antenna Measurements
> Overview
> Common RF Terms
> Overview
> What is Measured?
> Why Measure?
> Line Sweeping
> Calibration
> Line Sweep Measurements
> Return Loss/VSWR Measurement
> Cable Loss Measurement
> DTF Measurement
> Advanced Measurements
> Smith Chart
> 1-Port Phase
> Transmission (Ext. Sensor)
> Measurement Setup
> Frequency
> Distance
> Amplitude
> Sweep
> Limit Lines
> Markers
> Trace
> Measurement Review
> C&A Menus
> Measurement Menu
> Measurement Menu (Continued)
> Freq/Dist Menu
> Freq/Dist Menu (Continued)
> Windowing Menu
> Amplitude Menu
> Calibration Menu
> Marker Menu
> Marker Menu (Continued)
> Limit Menu
> Limit Menu (Continued)
> Sweep Menu
> Trace Menu
> Other Menus Keys
> Overview
> This chapter provides an overview of Cable and Antenna measurements and how to set up the instrument and perform basic line sweeps.

> Note | Use the Menu key and confirm that the instrument is in Cable & Antenna Analyzer Advanced mode (not Classic mode).

> Figure: Cable and Antenna Display Overview (1 of 2) illustrates a typical Cable and Antenna Return Loss measurement.

> Cable and Antenna Display Overview (1 of 2)
> 1 | Marker 1 (Marker to Peak)
> 2 | Active Trace (Yellow)
> 3 | Limit Line (Green when Passing)
> 4 | Measurement Type
> 5 | Marker 2 (Marker to Valley)
> 6 | Stop Frequency (F2)
> 7 | Pass Message (Active trace is below the limit line in Return Loss measurement)
> 8 | Marker Table
> 9 | Start Frequency
> 10 | Measurement Details (also Menu Shortcuts)
> 11 | User-defined Setup and Menu Shortcuts (not available in Classic mode)