> easyTest Tools
> easyTest Tools is used to create work instruction files that consist of a command sequence and intructions to help less experienced personnel with operating the instrument in the field.

> • | A drag-and-drop tool facilitates the creation of test scripts from a library of commands.

> • | Instructions can be a mix of text prompts and custom user images that may include connection diagrams or procedure steps.

> • | Recall Setup command lets you specify a particular setup, placing the instrument in a known state by retrieving saved parameters such as measurement type, frequency and amplitude settings, markers and limit lines.

> • | Measurements or screen shots can be saved automatically or manually.

> To recall an easyTest file:

> 1. | Press Menu on the S331L interface screen.

> 2. | Press the easyTest icon on the Menu Shortcut window.

> 3. | In the easyTest Recall dialog, select the .ett file and press Recall.

> easyTest Recall Dialog Box

> 4. | Press Next to move to the next instruction screen. To abort the easyTest sequence, press Esc.