> Battery Replacement
> The Site Master batteries are installed at the factory and can be replaced by the user.

> 1. | Power off the Site Master and remove the bottom bumper to expose the battery cover plate.

> 2. | Set the unit face up on a secure surface and remove the six (6) screws holding the battery cover plate ( Figure: Remove the Battery Cover Plate). Remove the cover plate and note the orientation for reassembly.

> Remove the Battery Cover Plate

> 3. | Carefully disconnect the battery connector and remove the battery. Repeat for the second battery ( Figure: Replacing the Batteries).

> Replacing the Batteries

> 4. | Slide the new batteries into the two battery bays and carefully plug in the battery connectors.( Figure: Adding the Second Battery).

> Adding the Second Battery

> 5. | Reattach the battery cover plate with the 6 six screws and put the bottom bumper back on the Site Master.