> Limit Menu
> Key Sequence: Limit or Limit (6)

> High Accuracy Power Meter Limit Menu

> Limit
> Turns the limits On or Off.
> Upper Value
> Sets the upper limit (displayed as red hash marks). Enter the desired number by using the keypad, the rotary knob, or the Up/Down arrow keys. If the keypad was used to enter new values, press Enter to set the new setting or press the Esc button to restore the previous setting.
> Lower Value
> Sets the lower limit (displayed as red hash marks). Enter the desired number by using the keypad, the rotary knob, or the Up/Down arrow keys. If the keypad was used to enter new values, press Enter to set the new setting or press the Esc button to restore the previous setting.