> Recall a Setup
> Setup files contain basic instrument setup details including: measurement type, frequency span, distance span, DTF setup, amplitude setting, markers, limit line, calibration coefficients, and additional instrument settings (data points, run/hold status). Recalling a setup may change the current settings.

> 1. | Press the File (1) key to display the File menu.

> 2. | Press Recall to open the Recall dialog box.

> 3. | Press the Filetype button, then touch Setup or All to list only setup files or all file types, respectively.

> 4. | Press the Location button and navigate to the desired setup file (.stp extension).

> 5. | Double-tap the file to recall the setup. Alternatively, you can press the file name to select, then press Enter (or Recall in the Recall dialog).

> Recall/Preview a Screen Shot

> 1. | Press the File (1) key to display the File menu.

> 2. | Press Recall to open the Recall dialog box.

> 3. | Press the Filetype button, then touch ScreenShot or All to list only screen shot files or all file types, respectively.

> 4. | Press the Location button and navigate to the desired screen shot file (.png extension).

> 5. | Select the file, then press Enter (or Recall in the Recall dialog). Alternatively, you can simply double-tap a file in the list to recall the screen shot.

> In the example below, the selected file is located in the default ScrnShots folder in the instrument internal memory.

> Screen Shot Selected for Recall

> 6. | A preview screen displaying the selected screen shot is illustrated in Figure: Preview of a Recalled Screen Shot. Press ESC to return to the File Recall menu.

> Preview of a Recalled Screen Shot