> Classic Mode Operation
> Introduction
> Marker Menu
> Marker Menu (Continued)
> Limit Menu
> Introduction
> The Site Master S331L features a Classic Cable and Antenna Analyzer measurement mode, which allows users of Site Master legacy series (up to series D) to become efficient immediately. To provide quick and easy familiarity with the Site Master user interface, many of the advanced features such as Dual Screen display, Smith Chart, Phase, and multi-segmented limits, are purposely removed while in Classic Mode. Please switch to Advanced Mode to access these useful features when desired.
> The primary purpose of Classic Mode is to help users of the S331L follow existing carrier’s Method of Procedure (MOP) documents while they become more familiar with the instrument. There are many additional features and capabilities in Advanced Mode that make the transition well worth the time to learn its intuitive operation.
> Figure: Display Appearance in Classic Mode vs. Advanced Mode illustrates the Site Master S331L screen display in Classic mode versus Advanced mode.

> Note | Use the Menu key and confirm that the instrument is in Classic Cable & Antenna Analyzer mode before continuing. Classic Mode will always be displayed above the measurement type when the instrument is in Classic mode.

> Many functions of the Site Master S331L are common between the Classic and Advanced measurement modes. Refer to Cable and Antenna Measurements for a complete overview of the instrument GUI.
> The Marker menu and the Limit menu in Classic mode are described Marker Menu andLimit Menu.

> Display Appearance in Classic Mode vs. Advanced Mode

> Descriptions of the main menus and associated submenus that are common between the Classic and Advanced measurement modes are provided in Cable and Antenna Measurements in Figure: Measurement Menu (1 of 2) through Figure: Trace Menu.

> Menu Differences Between Classic Mode and Advanced Mode
> Classic Mode | Advanced S331L Cable and Antenna Mode
> Mode Menu | Measurement Menu
> Freq - SWR | VSWR
> Freq - Return Loss | Return Loss
> Freq - Cable Loss (one port) | Cable Loss
> DTF - SWR | DTF VSWR
> DTF - Return Loss | DTF Return Loss
> — | Smith Chart
> — | 1-Port Phase
> Freq/Dist Menu | Freq/Dist Menu
> F1 | Start Frequency (F1)
> F2 | Stop Frequency (F2)
> D1 | Start Distance (D1)
> D2 | Stop Distance (D2)
> More | DTF Setup
> Meas/Disp Menu | Refer to Sweep Menu and Trace Menu
> Marker Menu
> Marker Menu | Marker Menu
> Limit Menu
> Limit Menu | Limit Menu

> Note | Also refer to Cable and Antenna Measurements for descriptions of other menus not specifically mentioned in Table 4-1.

> Figure: Classic Mode Menu Keys (1 of 2) and Figure: Classic Mode Menu Keys (2 of 2) show an overview of the Classic Cable and Antenna Analyzer menus.

> Classic Mode Menu Keys (1 of 2)

> Classic Mode Menu Keys (2 of 2)