> Q. My cable type does not show up in the cable list. What can I do?
> A: You can manually enter the cable information directly on the instrument anytime. Propagation Velocity and Cable Loss parameters may be entered via the DTF Aid menu.

> • | See Using DTF Aid for additional information.

> Also, users may add any custom cables to the standard list using the supplied PC software. Refer to the LST User Guide for specific instructions on modifying the built in cable list.